|  |  |
| --- | --- |
| **Customer information** | Date: |
| Company & dept.: | Contact person: |
| Address: | Telephone: |
| Zip code & city: | Mobile: |
| Country: | E-mail: |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Order information | | | | Order no.: |
| Other delivery address? | No | Yes **🡪** | Address: | |
| Other billing address? | No | Yes **🡪** | Address: | |
| Do you want shipping insurance? *\*Surcharge approx. 3-5 % of the stated value* | No | Yes\* **🡪** | Value: | |
| The items will be shipped to CemeCon on (date): by: | | | | |
| Desired delivery date / carrier: | | | | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Information on the items to be treated | | | | | | |
| Type of item: | | | Number of items: | | | |
| Material: | | | W.Nr.: | | | |
| Hardness (HCR): | | | Annealing/tempering temp (°C): | | | |
| Treatment of the item before arriving at CemeCon: | Spark eroded  Grinded | Micro blasted  Glass blasted | | Polished  High polished | Other: | |
| Item has been subjected to manufacturing processes: | Pressed  Welded | Soldered | | Glued | Other: | |
| Material to be worked (formed/cut/other) by item: | Stainless steel  Steel | Copper  Plastic | | Rubber  Aluminium | Other: | |
| Problems: | | | | | | |
| Wanted treatment: | I know what I want: | | | | | |
|  | HYPERLOX HT  HYPERLOX LT  HyperSlip TAN  TINALOX  +  TopFinish | TICANOX  TINALOX SN2  PureCr  HyperSlip PureCr | | UltraPlex HD  CrN  HyperSlip CrN | | TiN  DLC |
|  | CemeCon choose from the provided info  Please, call me for advice | | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| Sketch/picture of item | | |  |
| enclosed as an attachment / or drawn here **🡪** | | |
|  | | Surfaces to be treated |
|  | | Surfaces **not** be treated |
|  | | |
|  | | |
| **Billedresultat for exclamation mark** | **Do not use any adhesive tape or magic markers of any kind, especially on the functional surfaces. Remove the oxide layer created during tempering. Dismantle the items completely; items should be free of plugs and dividers / there should be passage through cooling channels. CemeCon charge an extra fee for additional services.** | | |